[How to use IQinVision ONVIF camera](#h.iuono4kt2vtn)

[How to use dual stream for Amegia camera](#h.9rp7bsim9lnf)

[How to use HUNT ONVIF cameras](#h.n9qev2kb5rzy)

[Event](#h.nksrvqjq5u2o)

[Dual stream](#h.5d0wx1monz26)

[How to use dual stream on Ingrasys iMege N3211E](#h.nuilmf6dll2u)

[How to enable ONVIF on ACTi cameras?](#h.qs8ri8f2r6u1)


[How to enable dual-streaming on EtroVision camera?](#h.i8kozmtten82)

[How to connect to A-MTK ONVIF camera?](#h.kzs2tkstqjgc)

[Configuration for Motion Detection](#h.3uyz63nuozkt)


## How to use IQinVision ONVIF camera

In CameraSetup, StreamUseTCP must be set to **yes** to see the video.



## How to use dual stream for Amegia camera

Check **Stream Enabled** in Setup page




## 

## 

## How to use HUNT ONVIF cameras


### Event

Set PullMessageTimeout to PT20S



### Dual stream

In **Video Setting**, enable **Streaming 2**




## How to use dual stream on Ingrasys iMege N3211E

Stream 2 in Video Setting must be enabled



## 


## How to enable ONVIF on ACTi cameras?



## 

## 

## How to enable dual-streaming on EtroVision camera?



## 

## 

## How to connect to A-MTK ONVIF camera?

The camera default username is “admin” and password is empty.


However for ONVIF function to work, the default username/password is different: “admin” for username, and “admin” for password.

### Configuration for Motion Detection

Motion Detection works only if it's configured as following…

1. Set Type to Entrance

2. Set Max. Inspection Trigger Size to cover whole image



3. Set Min. Inspection Trigger Size to 36x36

