# Camera Supporting Matrix

**Note**: Various [software version](https://docs.google.com/document/d/1HYOTyDtZog44dqUL3lv1-4lOZPaGG3QGag3VvS5ZG5s/pub), firmware version, and camera model combination may exhibit different level of support (or even non-support). If you are unsure, please [contact us](http://geniusvision.net/contact-us.html) to clarify the actual support of specific software version against specific camera model and features.

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

## 

## 

## Supported via ONVIF Verification

For more information, please visit [Free ONVIF Verification](http://geniusvision.net/onvif.html) and [ONVIF Camera Matrix](https://docs.google.com/spreadsheet/pub?key=0AnmAMRiHiy2fdDNnNmVJanNveWJUcVNmM2RhQ0dPaHc&output=html).

|  |  |  |  |
| --- | --- | --- | --- |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |
|  |  |  |  |

## 

**- Index -**

[Camera Supporting Matrix](#h.kr0t6y2i7egp)

[AXIS](#h.ho6mq6paby1)

[Arecont Vision](#h.9372bcgihks3)

[A-MTK](#h.uq96csnobz4)

[AirLive](#h.m59s2j4tqja)

[StarDot](#h.812kfjric70s)

[IQinVision](#h.uqdaiqzdb41x)

[VIVOTEK](#h.ymacr5opo8je)

[SONY](#h.kv3bmz6bnxa7)

[ACTi](#h.mmj986tl46zs)

[Brickcom](#h.20pwkmwgm2ve)

[Panasonic](#h.5sjvt2c99id9)

[PIXORD](#h.dersh8gpuffo)

[Truen](#h.r9tq8hg62bmi)

[JVC (V.Networks)](#h.dsnct6mm50y3)

[LILIN](#h.awsaje30q63s)

[Asoni](#h.vbd1rnf14n7p)

[ZAVIO](#h.vmamerrys4dl)

[CTC-U](#h.6qsdv8plne4d)

[EtroVision](#h.f2jcje4og8my)

[BOSCH (VideoJet)](#h.72fv2xubwei4)

[SHANY](#h.xfab32sank4d)

[MatriCam](#h.y7sgps7wkxia)

[ONVIF](#h.2lunkbymucq)

[WebCam (DirectShow)](#h.xkb116rwatec)

[Foscam](#h.gpozv5q5b7d)

[GeoVision](#h.yx5fz1hi52rl)

[iPUX](#h.ahseidx0y4sw)

[RTSP Supporting Information](#h.vd9rs6r8qf2q)

[AVI-Export Supporting Information](#h.e37wi5ods6i4)

## 

## AXIS

**Supported Features**

* Video: H.264, M-JPEG, [RTSP](#id.9zn1f3u8zuxy)
* Audio:[RTSP](#id.9zn1f3u8zuxy)
* Video parameters setup
* Motion event/setup
* Pan-Tilt-Zoom with 8 directions and free mode.
* Preset set/recall.
* Focus control.
* Digital input/output.
* Audio out (two-way).
* Auto discovery.

**Supported Models**

* M1011, M1011-W, M1031-W, M1054, M1103, M1104, M1113, M1114, P1311, P1343, P1344, P1346, P1347, P1343-E, P1344-E, P1346-E, P1347-E, Q1755, Q1755-E, 211W, 221, M3011, M3014, M3113-R, M3114-R, M3203, M3204, M3203-V, M3204-V, P3343, P3344, P3346, P3343-V, P3344-V, P3346-V, P3343-VE, P3344-VE, P3346-VE, P3301, P3304, P3301-V, P3304-V, 209FD, 216FD, 216FD-V, 216MFD, 216MFD-V, 212PTZ, 212PTZ-V, 214PTZ, 215PTZ, 215PTZ-E, P5512, P5522, P5512-E, P5522-E, Indoor, P5532, P5534, P5532-E, P5534-E, Q6034, Q6032-E, Q6034-E, Q1910, Q1921, Q1910-E, Q1921-E, 233D, Q6034, Q6032-E, Q6034-E, 241S, 243SA, 247S, Q7401, M7001, M7001, 240Q, 241Q, 241QA, 243Q Blade, Q7406 Blade, Q7404, 291 1U, Q7900,

**Related Information**

* [AXIS Application Developer Partner - Taiwan](http://www.axis.com/zh/partner/adp/result.php?cc=tw)

## Arecont Vision

**Supported Features**

* Video: M-JPEG, H.264
* Video parameters setup

**Supported Models**

* AV10005, AV2805, AV1305, AV1355, AV1300, AV1310, AV2105, AV2155, AV2100, AV2110, AV3105, AV3155, AV3100, AV3110, AV5105, AV5155, AV5100, AV5110, AV3130, AV3135, AV8185DN, AV8365DN, AV8185, AV8180, AV8365, AV8360, AV1315, AV2815, AV1325, AV2825,

## A-MTK

**Supported Features**

* Video: M-JPEG, MPEG4, H.264, RTSP
* Auto discovery
* Digital input/output
* PTZ control

**Supported Models**

* (TBW)

## AirLive

**Supported Features**

* Video: M-JPEG, MPEG4, H.264, RTSP
* Auto discovery
* Digital input/output
* PTZ control

**Supported Models**

* OD-2025HD, OD-2025PHD, WN-2600HD, POE-2600HD, OD-2060HD, OD-2050HD, IP-200PHD-24, WN-200HD, CU-720PIR, CW-720

**Minimum Supported Software Version**

* b70: Version 772

## StarDot

**Supported Features**

* Video: M-JPEG, H.264,[RTSP](#id.9zn1f3u8zuxy)
* Video parameters setup
* Motion event/setup
* Auto discovery.
* Digital input/output

**Supported Models**

* ExpressXL series, NetCamXL series, NetCamSC series, NetCamSCD series

## IQinVision

**Supported Features**

* Video: M-JPEG,
* Motion event.

**Supported Models**

* IQ755, IQ753

## VIVOTEK

**Supported Features**

* Video: M-JPEG, MPEG-4, H.264
* Audio: AAC, AMR
* Motion event/setup.
* Pan-Tilt-Zoom with 4 directions.

**Supported Models**

* IP8362, IP8162P, IP8162, IP8151P, IP8151, IP7361, IP7142, IP8332, IP8330, IP7330, IP8161, IP7161, IP7160, IP7154, IP7153, IP7130, IP8132, IP7134, IP7133, PZ71x2, PZ71x1, PZ7152, PZ7151, PZ7132, PZ7131, PT7137, PT7135, SD73x3, SD7151, SD81x1, FD8361, FD8361L, FD7141, FD8161, FD7132, FD7131, MD7560, MD7530, FD8134V, FD8133V, FD8134, FD8133, IP8352, FE8171V, SD8362E, SD83x3E, SD83x2E, SD83x1E, FD8362E, FD8362, FD8162,

## SONY

**Supported Features**

* Video: M-JPEG, MPEG-4, H.264
* Audio: G.711, G.726
* Motion event/setup. (Not all models are supported. Known supported models are RZ50, RX550)
* Pan-Tilt-Zoom with 8 directions.

**Supported Models**

* SNC-RZ50N, SNC-RZ30, SNC-P5, SNC-RX550, SNC-P1

## ACTi

**Supported Features**

* Video: MPEG-4
* Audio: PCM 16K
* Video parameters setup
* Motion event/setup.
* Pan-Tilt-Zoom with 8 directions.
* Preset set/recall.
* Digital input/output.

**Supported Models**

* ACM-5001, ACM-5601, ACM-5611, KCM-5111, KCM-5211, KCM-5311, TCM-5311, TCM-5601, TCM-5611, ACM-1231, ACM-1431, TCM-1231, TCM-1511, ACM-4001, ACM-4201, TCM-4201, ACM-3001, ACM-3011, ACM-3401, ACM-3411, ACM-3511, ACM-3601, ACM-3701, ACM-7411, KCM-7111, KCM-7211, TCM-3401, TCM-3411, TCM-3511, TCM-7411, TCM-7811, ACM-8511, CAM-6610, CAM-6630, ACD-2000Q, ACD-2100, ACD-2200, ACD-2300, ACD-2400, TCD-2100, TCD-2500,

## Brickcom

**Supported Features**

* Video: H.264, [RTSP](#id.9zn1f3u8zuxy)
* Audio:[RTSP](#id.9zn1f3u8zuxy)
* Video parameters setup
* Dual (multiple) streaming.
* Audio out (two-way).
* Digital input/output
* Auto discovery.

**Supported Models**

* CB-102A Series, CB-101A Series, FB-300A Series
* FB-130N Series, FB-130A Series, FB-100A Series
* FD-130A Series, FD-100A Series, MD-100A Series
* OSD-040 36x Series, PZ-040 12x Series
* VD-130A Series, VD-100A Series

**Related Information**

* [Brickcom IP Cameras Integrated with Genius Vision NVR](http://www.brickcom.com/news/press-release_detailview.php?id=99)

**Minimum Supported Software Version**

* b60: Version 610
* b70: All

## Panasonic

**Supported Features**

* Video: H.264,[RTSP](#id.9zn1f3u8zuxy)
* Audio:[RTSP](#id.9zn1f3u8zuxy)
* Video parameters setup
* Pan-Tilt with 4 directions and click-move-to.
* Preset set/recall.
* Focus control.
* Dual (multiple) streaming.

**Supported Models**

* BL-C2xx: BL-C230A/C210A
* BL-C1xx: BL-C121A/C101A,C160A/C140A,C131A/C111A
* BB-HCM7xx: BB-HCM701A/HCM705A,HCM735A/HCM715A
* BB-HCM5xx: BB-HCM547A/HCM527A/HCM581A/HCM580A/HCM531A/HCM511A/HCM515A

## PIXORD

**Supported Features**

* Video: H.264, [RTSP](#id.9zn1f3u8zuxy)
* Audio: [RTSP](#id.9zn1f3u8zuxy)
* Video parameters setup
* Digital input/output.

**Supported Models**

* PD636, PD634, PB630(W), PD637, P600, P606(W), PD614, P-415M, P-416(W), P-413, P-400(W), P-426, P-412, P-405(W), PL621, P-423, P-428, P-465, P463A, P463H, P600E, PD634E, P-400 PoE, P-426 PoE, P-413 PoE, PL621E, P-423 PoE, PV6901, P-1401 (W,PoE), P-4000,

## Truen

**Supported Features**

* Video: H.264, [RTSP](#id.9zn1f3u8zuxy)
* Audio: [RTSP](#id.9zn1f3u8zuxy)
* Video parameters setup
* Digital input/output.
* Motion event and setup.
* Dual (multiple) streaming

## JVC (V.Networks)

**Supported Features**

* Video: M-JPEG
* Pan-Tilt-Zoom with 8 directions and click-move-to.
* Preset set/recall.

**Supported Models**

* C30U, C625U, C655U,
* VN-V685U, VN-686U, VN-686BU

## LILIN

**Supported Features**

* Video: H.264, M-JPEG, [RTSP](#id.9zn1f3u8zuxy)
* Audio: [RTSP](#id.9zn1f3u8zuxy)
* Pan-Tilt-Zoom with 8 directions.
* Preset set/recall.
* Auto discovery.

**Supported Models**

* IPD552EX, IPR454, IPR458, IPS203, IPS212, IPS303, IPS312, IPS125, IPS130, IPS135,
* IPS025, IPS030, IPS035, IPG012ES, IPD112ESX, IPR312SX, IPR614ES, IPR618ES, IPR414ESX, IPR418ESX, IPR712S, VS012, BTE02S,

**Related Information**

* [LILIN IP Surveillance Software Partner](http://www.meritlilin.com/en/alliance2.asp)
* [LILIN ONVIF/HTTPAPI VMS Software Feature Support Matrix](http://www.meritlilin.com/data/product/common/Q00043LILIN_ONVIF_Support_List.pdf)

## Asoni

**Supported Features**

* Video: H.264, M-JPEG, [RTSP](#id.9zn1f3u8zuxy)
* Audio: [RTSP](#id.9zn1f3u8zuxy)
* Video parameters setup
* Motion event and setup
* Digital input/output.
* Pan-Tilt with 4 directions.
* Preset set/recall.
* Focus control.
* Auto discovery.

**Supported Models**

* CAM4xx series, CAM6xx series, CAM7xx series

## ZAVIO

**Supported Features**

* Video: MPEG-4, [RTSP](#id.9zn1f3u8zuxy)
* Audio:G.711, [RTSP](#id.9zn1f3u8zuxy)
* M-JPEG
* Video parameters setup
* Pan-Tilt-Zoom (8 directions)
* Preset set/recall.
* Focus control.
* Digital input/output.

**Supported Models**

* F210A, F312A, F3100, F3105, F3101, F3106, F7110, F7115, B5110, F531E, F731E, D5110, D5111, D7110, M511E, M511W, P5110, P5115, V111T

## CTC-U

**Supported Features**

* Video: H.264, [RTSP](#id.9zn1f3u8zuxy)
* Audio: [RTSP](#id.9zn1f3u8zuxy)
* Pan-Tilt zoom (8 directions)
* Preset set/recall.
* Focus control.
* Digital input/output.
* Auto discovery.

**Supported Models**

* DVS-8501E, DVS-8501E-H, DVS-8504E-FD, DVS-8504E-H, DVS-8301, IPCAM-8318P, IPCAM-8318F, IPCAM-8309D, IPCAM-8309FW, IPCAM-8309F,

## EtroVision

**Supported Features**

* Video: MPEG-4, H.264
* Video parameters setup
* Pan-Tilt-Zoom with 4 directions
* Preset set/recall
* Focus control

## BOSCH (VideoJet)

**Supported Features**

* Video: M-JPEG
* Pan-Tilt with 8 directions

**Supported Models**

* VideoJet-10

## SHANY

**Supported Features**

* Video: H.264, M-JPEG, [RTSP](#id.9zn1f3u8zuxy)
* Audio: G.711, [RTSP](#id.9zn1f3u8zuxy)
* Video parameters setup.
* Auto discovery.
* Dual (multiple) streaming.
* Digital input/output.
* Pan-Tilt-Zoom with 8 directions

**Supported Models**

* IP Megapixel Camera: SNC-WD2312MDN, SNC-WD2312DN, SNC-WD2322DN, SNC-WD2332DN, SNC-2212DN, SNC-2252DN, SNC-2222DN, SNC-WD2112MDN, SNC-WD2112DN, SNC-WD2152MDN, SNC-WD2122DN, SNC-WD2132DN, SNC-WDL2122DN, SNC-WDL2132DN, SNC-WDL2142DN,
* IP Camera: SNC-WD1010MDN, SNC-1010MDN, SNC-1020DN, SNC-1030DN, SNC-L1023DN, SNC-L1040M, SNC-91IR26DN, SNC-81IR26DNS, SNC-81IR26DNC, SNC-82IR26DN

**Related Information**

* [SHANY 3rd party NVR](http://www.shany.com/p03-0a15.htm)

**Minimum Supported Software Version**

* b70: Version 743

## MatriCam

**Supported Features**

* Video/Audio: [RTSP](#id.9zn1f3u8zuxy)
* Video parameters setup.
* Auto discovery.
* Dual (multiple) streaming
* Audio out (two-way).
* Digital input/output.

**Minimum Supported Software Version**

* b70: Version 725

## ONVIF

**Supported Features**

* Video/Audio: [RTSP](#id.9zn1f3u8zuxy)
* Auto discovery.
* Video parameters setup.
* Dual streaming (after 841)

**Minimum Supported Software Version**

* b60: Version 633
* b70: All

## WebCam (DirectShow)

**Supported Features**

* Video: DirectShow YV12/M-JPEG
* Audio: Generic PC audio
* Auto discovery.
* Software compression: JPEG/MPEG-4

## Foscam

**Supported Features**

* Video:M-JPEG

**Minimum Supported Software Version**

* b60: Version 656
* b70: Version 761

## GeoVision

**Supported Features**

* Video:H.264, M-JPEG
* Dual streaming.
* Video parameters setup.
* Auto discovery. (UPnP)

**Minimum Supported Software Version**

* b80: Version 838
* b70: Version 790

## iPUX

**Supported Features**

* Video:H.264, M-JPEG
* Dual streaming.
* Video parameters setup.
* Auto discovery.

**Minimum Supported Software Version**

* b80: Version 838
* b70: Version 780

# 

# RTSP Supporting Information

**Supported Video Codecs**

* MPEG-4
* M-JPEG
* H.264

**Supported Audio Codecs**

* G.711
* AAC
* AMR
* G.726
* MPEG audio

**Supported Transport Modes**

* UDP
* TCP
* HTTP

See also

* [Adding RTSP camera](https://docs.google.com/document/d/1cOlmrzZ3ducWzDZgPGyJpXHPhTSsiU4q_P9atw3ZmRM/pub#kix.jnt0pyaw5khg)

# 

# 

# AVI-Export Supporting Information

**Supported Video Codecs**

* MPEG-4
* M-JPEG
* H.264

**Supported Audio Codecs**

* G.711
* PCM